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Three-layer automatic production line for cast and stretch film

1. Manufacturer: DLOCI EXTRUSION
2. Type: CAST FCL21-BICONTAX
3. Serial number: UZ 3124/04
4. Year of manufacture: 2004. Refurbished in 2008.
5. Materials: Homopolymer, copolymer.
6. Capacity: CCP – 450 kg/h; Stretch – 650 kg/h. 
- Thickness range: 15–37 microns (stretch film), 15–60 microns (cast film).
6. Technical specifications:
- Installed power: 665 kW
- Chiller: 113 kW (300,000 kcal), operating range 7–12°C. 
- Extruders: 75–140–75, L/D ratio 1:30. 
- Filters: Hydraulic (manual operation). 
- Feeding system: DOTECO + 4-component dosing unit for the homopolymer. 
- Automatic die: SIMPLAS, 2550 mm, equipped with thermal bolts. 
- Thickness measurement and control: Automatic, via ELECTRONIC SYSTEMS – SINTEL 9000.
- Chill roll unit: 1st roll Ø 800 mm x 2500 mm; 2nd roll Ø 350 mm x 2500 mm. 
- Edge guiding system: Fife – Tidland GmbH.
- Corona treatment: FERRARINI & BENELLI.
- Automatic winding with 4-lane slitting; compatible with Ø 76 mm and Ø 150 mm cores. Max. diameter for CPP: 800 mm; for stretch film: 500 mm. Maximum speed: 350 m/min. 
- Edge trim granulator – automatic feeding of trim scrap into the main extruder via an auxiliary extruder (R).
- Maximum product width: 2000–2100 mm (net).
- Thickness range: 18–60 microns.
7. Electrical system
- ABB DC motors with Control Techniques drives
- ABB AC motors
- ABB tension control
- SIEMENS S7 thermal control
- SIEMENS S7 PLC








Three-layer extrusion line for the production of cast and stretch film, manufactured in Italy in 2004. Commissioned in 2005. Maximum output capacity is up to 1000 kg/h, depending on the thickness of the film being produced. Actual production rates are 500 kg/h for cast film and 650 kg/h for stretch film. Winding speed for the finished products is up to 350 m/min. Thickness range: 15–37 microns for stretch film and 15–60 microns for cast film. Film width: 2100 mm. The film structure is A/B/C, with layer ratios of 15/70/15 or 20/60/20.

Line configuration: Includes three extruders (diameters 75–140–75 mm), type DE-KC. Each extruder is equipped with a Doteco feeding system; the main extruder features a four-component dosing unit, allowing for the addition of up to four components (including masterbatch). The extruders are equipped with hydraulic screen changers.
The line also includes:
A three-layer co-extrusion block where the film structure is formed; an extrusion die with thermal bolts; a film cooling module consisting of two chill rolls; a vacuum system for adhering the film to the chill roll; and devices for the electrostatic pinning of the film edges. A system for measuring the thickness of the produced film, linked to thermal bolts mounted on the extruder die head. This allows for automatic thickness adjustment during production. Features include an edge-tracking system, corona treatment, and a winding unit for the finished product—which also performs cutting to the required dimensions—along with an automatic roll-changing system. Edge trim is recovered via a mill and granulator system positioned at a 90-degree angle to the main extruder, allowing for 100% recycling of the trim.
The machine has not been in operation since 2024 but remains in working condition. A test run can be arranged under specific conditions.

Price: €750,000 (negotiable).
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PRODUCTION AND TRADING WITH POLYMERIC PACKAGES AND FILMS
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