1. Wity / Ruihua XSH-1515/6 (Large Format)
• Forming Area: 1500 x 1500 mm
• Max. Mold Height: 650 mm
• Sheet Thickness: 1 – 10 mm
• Materials: ABS, HDPE, LDPE, PP, PVC, PMMA, HIPS
• Heating: Upper & lower infrared ceramic heaters with separate multi-zone control cabinet
• Control: Siemens PLC with Siemens Simatic Multi Panel Touch Screen
• Vacuum: Becker industrial vacuum pump + vacuum reservoir tank
• Price: €35,000 net (EXW Hungary)

The machines can be inspected and test-run under power. Operation videos, extra photos, and full manuals are available upon request. We can also assist with loading and export formalities.[image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ]
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